* ATC/TTC Declaration of BSPTCL System for the following months is as mentioned below:-

|  |  |  |  |
| --- | --- | --- | --- |
| Month | TTC (MW) | ATC(TTC-RM)(MW) | RM(MW) (2% of peak demand) |
| April-2023 | 6531 | 6400 | 131 |

TTC-Total Transfer capability

ATC-Available Transfer capability

RM-Reliability Margin

RM-Reliability Margin (2% of peak demand or maximum generation in the state)

Taking 2% of Peak demand as reliability margin.

ATC=TTC-RM

|  |
| --- |
| **Assumptions** |
| Month | Generation (MW) (Including Thermal & Hydro generator of central sector & Sate sectors) | Peak Load(MW) | Remarks |
| April-2023 | 7526 | 6400 | Total LTA of BSPHCL with Thermal & Hydro generator of central sector & Sate sectors is of 7526MW |
|  |
| **Constraints** |
| No any constraint at this loading condition. |

`