|  |  |  |  |
| --- | --- | --- | --- |
| **Assumptions** | | | |
| Month | Generation (MW) (Including central sector & Sate generation) | Peak Load(MW) | Remarks |
| Aug-2020 | **4579.51** | 6390 | Total LTA of BSPHCL with Central Sector & State generators is of 5269.51 MW but among the state generators only one unit of of NTPC Barauni (1\*250MW) generally remain in service. |
| Sep-2020 | 6450 |
| **Constraints** | | | |
| 1.Following Trans. Lines get overloaded  i) 132Kv Sone nagar-Sone nagar New D/C T/L  ii) 132KV Laukahi-Phoolparas T/L  iii) 132 KV Ramnagar-Narkatiyaganj-Bettiah T/L | | | |